Slow Extraction beam quality of circulating cooled beam at low energies limited by residual gas pressure methods: by electron capture

in electron cooler in gas target by ionization in gas target for both modes: extraction rates of 10^{- 3}- 10^{- 1}s^{- 1}

by resonance extraction (not tested,

maybe difficult with cooled beam)