Transverse Beam Size determined by scraping